%
% Technische Informatik
\newacronym[
  description=Application Specific Standard Product
]{assp}{ASSP}{application specific standard product}
\newacronym[
  description=Application Specific Integrated Circuit
]{asic}{ASIC}{application specific integrated circuit}
\newacronym[
  description=Configurable Logic Block
]{clb}{CLB}{configurable logic block}
\newacronym[
  description=Complementary Metal-Oxide-Semiconductor
]{cmos}{CMOS}{complementary metal-oxide-semiconductor}
\newacronym[
  description=Complex Programmable Logic Device
]{cpld}{CPLD}{complex programmable logic device}
\newacronym[
  description=Erasable Programmable Read Only Memory
]{eprom}{EPROM}{erasable programmable read only memory}
\newacronym[
  description=Electrically Erasable Programmable Read Only Memory
]{eeprom}{EEPROM}{electrically erasable programmable read only memory}
\newacronym[
  description=Field Programmable Gate Array
]{fpga}{FPGA}{field programmable gate array}
\newacronym[
  description=Generic Array of Logic
]{gal}{GAL}{generic array of logic}
\newacronym[
  description=Hardware Description Language
]{hdl}{HDL}{hardware description language}
\newacronym[
  description=Integrated Circuit
]{ic}{IC}{integrated circuit}
\newacronym[
  description=Input/Output
]{io}{I/O}{input/output}
\newacronym[
  description=Look-Up-Table
]{lut}{LUT}{look-up-table}
\newacronym[
  description=Microcontroller
]{mcu}{MCU}{microcontroller}
\newacronym[
  description=One-Time-Programmable
]{otp}{OTP}{one-time-programmable}
\newacronym[
  description=Programmable Array Logic
]{pal}{PAL}{programmable array logic}
\newacronym[
  description=Programmable Logic Arrays
]{pla}{PLA}{programmable logic arrays}
\newacronym[
  description=Programmable Logic Device
]{pld}{PLD}{programmable logic device}
\newacronym[
  description=Programmable Read Only Memory
]{prom}{PROM}{programmable read only memory}
\newacronym[
  description=Simple Programmable Logic Device
]{spld}{SPLD}{simple programmable logic device}
\newacronym[
  description=Static Random-Access Memory
]{sram}{SRAM}{static random-access memory}
\newacronym[
  description=Very High Speed Integrated Circuit HDL
]{vhdl}{VHDL}{very high speed integrated circuit HDL}
%
% Mechatronik
\newacronym[
  description=Analog-to-Digital Converter
]{adc}{ADC}{analog-to-digital converter}
\newacronym[
  description=Active Noise Control
]{anc}{ANC}{active noise control}
\newacronym[
  description=Digital-to-Analog Converter
]{dac}{DAC}{digital-to-analog converter}
\newacronym[
  description=Digital Signal Processing
]{dsp}{DSP}{digital signal processing}
\newacronym[
  description=Finite Impulse Response
]{fir}{FIR}{finite impulse response}
\newacronym[
  description=Infinite Impulse Response
]{iir}{IIR}{infinite impulse response}
\newacronym[
  description=Multiple-Input and Multiple-Output
]{mimo}{MIMO}{multiple-input and multiple-output}
\newacronym[
  description=Filtered-x LMS
]{fxlms}{FXLMS}{filtered-x LMS}
\newacronym[
  description=Least Mean Square
]{lms}{LMS}{least mean square}
% Wirtschaft
